SmartShow Pro-ONE Firmware Update Information

IMPORTANT : Please ensure you plug the Pro-ONE directly into your PC/Laptop using a quality USB-A to USB-Mini cable (do not use a USB Hub)

Please download and unzip this firmware update for the SmartShow Pro-ONE. 
You can run the updater by firstly plugging the Pro-ONE in via USB to a windows machine, then double-clicking the "Pro-ONE_vx.xx FIRMWARE.bat" file.
Then type in the suggested com port and press ENTER. 
The firmware should automatically upload and reboot the Pro-ONE once complete
You can check the update has been successfully applied by accessing the WebUI and checking the firmware version written at the bottom of the page. 

Additional Notes
1. Some computers require elevated permissions. If you see a permissions error, right click on the .BAT file and select "Run as Administrator".
2. This firmware upgrade will not reset your settings. If your controller was in 32U Extended mode prior to the upgrade, you will have to put the controller into configuration mode to access the webUI.

If you have any issues, please contact us at sales@smartshow.lighting
